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[bookmark: whats_in_the_box]What’s in the box
· ☒ Lumen T2 printer
· ☒ USB-C cable (1 m)
· ☒ Power adapter, 24 V
· ☒ One roll of 50 × 30 mm labels
Warning
Use only the power adapter supplied with the printer. Other adapters can damage the print head.
[bookmark: setting_up]Setting up
1. Open the top cover by pressing the release button on the right side.
1. Load the label roll with the labels facing up, and pull about 5 cm through the slot.
1. Close the cover until it clicks. The printer feeds one label to find the gap.
1. Connect the power adapter and press the power button for two seconds.
[image: /var/folders/bl/5n_h09gn4dsd1gktj5qcv54w0000gn/T/docforge-bhj3mv0n/media-docx/image1.png]
[bookmark: ref_fig1]Figure 1. The status light during setup
[bookmark: printing_your_first_label]Printing your first label
Install the Lumen app, then add the printer:
Settings → Printers → Add → Lumen T2
Tip
Hold the feed button for three seconds to print a test label with the printer’s settings.
[bookmark: specifications]Specifications
[bookmark: table1]Table 1. Lumen T2 specifications
	Item
	Value

	Print method
	Direct thermal

	Resolution
	300 dpi

	Print speed
	up to 150 mm/s

	Label width
	20–60 mm

	Connection
	USB-C, Wi-Fi 2.4 GHz

	Size
	118 × 96 × 82 mm


[bookmark: status_light]Status light
	Light
	Meaning
	What to do

	Green
	Ready
	—

	Blinking green
	Printing
	Wait

	Orange
	Out of labels or cover open
	Load labels, close the cover

	Red
	Print head too hot
	Pause for five minutes
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